* **R11**

en

conf term

hostname R11

no ip domain-lookup

service password-encryption

security passwords min-length 10

login block-for 120 attempts 3 within 60

enable password cisco54321

enable secret cisco12345

banner login #Accesul persoanelor neautorizate interzis!#

banner motd #Vineri la ora 16 serverul intra in mentenanta!#

line console 0

password ciscoconpass

login

logging synchronous

exec-timeout 0 0

line vty 0 15

password ciscovtypass

login

logging synchronous

exec-timeout 0 0

no cdp run

interface gig0/1

no sh

ip add 172.16.0.9 255.255.255.252

description "legatura cu PC1"

interface gig0/0

no sh

ip add 192.168.0.14 255.255.255.252

description "legatura cu R1"

================static===============

ip route 0.0.0.0 0.0.0.0 gig0/0

=====================================

================R11===============

conf t

router ospf 1

network 172.16.0.8 0.0.0.3 area 10

network 192.168.0.12 0.0.0.3 area 10

=====================================

===================RIPv2==================

conf t

router rip

version 2

no auto-summary

network 172.16.0.0

network 192.168.0.0

=====================================

==============EIGRP=============

conf t

router eigrp 12

no auto-summary

network 172.16.0.8 0.0.0.3

network 192.168.0.12 0.0.0.3

do wr

=================================

do wr

* **R1**

================R1===============

ip route 0.0.0.0 0.0.0.0 gig0/0

ip route 172.16.0.8 255.255.255.252 gig0/2

=====================================

================R1===============

conf t

router ospf 1

network 10.0.0.28 0.0.0.3 area 10

network 10.0.0.92 0.0.0.3 area 10

network 192.168.0.12 0.0.0.3 area 10

=====================================

================RIPv2=====================

conf t

router rip

version 2

no auto-summary

network 10.0.0.0

network 192.168.0.0

=====================================

==============EIGRP=============

conf t

router eigrp 12

no auto-summary

network 10.0.0.28 0.0.0.3

network 10.0.0.92 0.0.0.3

network 192.168.0.12 0.0.0.3

do wr

=================================

do wr

* **R2**

en

conf term

hostname R2

no ip domain-lookup

service password-encryption

security passwords min-length 10

login block-for 120 attempts 3 within 60

enable password cisco54321

enable secret cisco12345

banner login #Accesul persoanelor neautorizate interzis!#

banner motd #Vineri la ora 16 serverul intra in mentenanta!#

line console 0

password ciscoconpass

login

logging synchronous

exec-timeout 0 0

line vty 0 15

password ciscovtypass

login

logging synchronous

exec-timeout 0 0

no cdp run

interface gig0/2

no sh

ip add 192.168.0.29 255.255.255.252

description "legatura cu R21"

interface gig0/0

no sh

ip add 10.0.0.30 255.255.255.252

description "legatura cu R1"

interface gig0/1

no sh

ip add 10.0.0.61 255.255.255.252

description "legatura cu R3"

================R2===============

ip route 0.0.0.0 0.0.0.0 gig0/1

ip route 172.16.0.16 255.255.255.252 gig0/2

=====================================

================R2===============

conf t

router ospf 1

network 10.0.0.28 0.0.0.3 area 10

network 10.0.0.60 0.0.0.3 area 10

network 192.168.0.28 0.0.0.3 area 10

=====================================

================RIPv2=====================

conf t

router rip

version 2

no auto-summary

network 10.0.0.0

network 192.168.0.0

=====================================

==============EIGRP=============

conf t

router eigrp 12

no auto-summary

network 10.0.0.28 0.0.0.3

network 10.0.0.60 0.0.0.3

network 192.168.0.28 0.0.0.3

do wr

=================================

do wr

* **R21**

en

conf term

hostname R21

no ip domain-lookup

service password-encryption

security passwords min-length 10

login block-for 120 attempts 3 within 60

enable password cisco54321

enable secret cisco12345

banner login #Accesul persoanelor neautorizate interzis!#

banner motd #Vineri la ora 16 serverul intra in mentenanta!#

line console 0

password ciscoconpass

login

logging synchronous

exec-timeout 0 0

line vty 0 15

password ciscovtypass

login

logging synchronous

exec-timeout 0 0

no cdp run

interface gig0/1

no sh

ip add 172.16.0.17 255.255.255.252

description "legatura cu PC2"

interface gig0/0

no sh

ip add 192.168.0.30 255.255.255.252

description "legatura cu R2"

================static===============

ip route 0.0.0.0 0.0.0.0 gig0/0

=====================================

================R21===============

conf t

router ospf 1

network 172.16.0.16 0.0.0.3 area 10

network 192.168.0.28 0.0.0.3 area 10

=====================================

===================RIPv2==================

conf t

router rip

version 2

no auto-summary

network 172.16.0.0

network 192.168.0.0

=====================================

==============EIGRP=============

conf t

router eigrp 12

no auto-summary

network 172.16.0.16 0.0.0.3

network 192.168.0.28 0.0.0.3

do wr

=================================

do wr

* **R3**

en

conf term

hostname R3

no ip domain-lookup

service password-encryption

security passwords min-length 10

login block-for 120 attempts 3 within 60

enable password cisco54321

enable secret cisco12345

banner login #Accesul persoanelor neautorizate interzis!#

banner motd #Vineri la ora 16 serverul intra in mentenanta!#

line console 0

password ciscoconpass

login

logging synchronous

exec-timeout 0 0

line vty 0 15

password ciscovtypass

login

logging synchronous

exec-timeout 0 0

no cdp run

interface gig0/2

no sh

ip add 192.168.0.45 255.255.255.252

description "legatura cu R31"

interface gig0/0

no sh

ip add 10.0.0.94 255.255.255.252

description "legatura cu R1"

interface gig0/1

no sh

ip add 10.0.0.62 255.255.255.252

description "legatura cu R2"

================R3===============

ip route 0.0.0.0 0.0.0.0 gig0/0

ip route 172.16.0.24 255.255.255.252 gig0/2

=====================================

================R3===============

conf t

router ospf 1

network 10.0.0.92 0.0.0.3 area 10

network 10.0.0.60 0.0.0.3 area 10

network 192.168.0.44 0.0.0.3 area 10

=====================================

================RIPv2=====================

conf t

router rip

version 2

no auto-summary

network 10.0.0.0

network 192.168.0.0

=====================================

==============EIGRP=============

conf t

router eigrp 12

no auto-summary

network 10.0.0.60 0.0.0.3

network 10.0.0.92 0.0.0.3

network 192.168.0.44 0.0.0.3

do wr

=================================

do wr

* **R31**

en

conf term

hostname R31

no ip domain-lookup

service password-encryption

security passwords min-length 10

login block-for 120 attempts 3 within 60

enable password cisco54321

enable secret cisco12345

banner login #Accesul persoanelor neautorizate interzis!#

banner motd #Vineri la ora 16 serverul intra in mentenanta!#

line console 0

password ciscoconpass

login

logging synchronous

exec-timeout 0 0

line vty 0 15

password ciscovtypass

login

logging synchronous

exec-timeout 0 0

no cdp run

interface gig0/1

no sh

ip add 172.16.0.25 255.255.255.252

description "legatura cu PC3"

interface gig0/0

no sh

ip add 192.168.0.46 255.255.255.252

description "legatura cu R3"

================static===============

ip route 0.0.0.0 0.0.0.0 gig0/0

=====================================

================R31===============

conf t

router ospf 1

network 172.16.0.24 0.0.0.3 area 10

network 192.168.0.44 0.0.0.3 area 10

=====================================

===================RIPv2==================

conf t

router rip

version 2

no auto-summary

network 172.16.0.0

network 192.168.0.0

=====================================

==============EIGRP=============

conf t

router eigrp 12

no auto-summary

network 172.16.0.24 0.0.0.3

network 192.168.0.44 0.0.0.3

do wr

=================================

do wr